## Operating Instructions – Umote Remote Control

### Normal Operation

1. Switch on without pressing any of the Umote buttons.
2. Each button will light in sequence to indicate normal mode.
3. Ensure Umote is pointing at the device to be controlled
4. Press the button for the required function. This must be programmed before it can be used (see below).
5. Button will light for a short time. When button turns off the next button can be pressed.

### Programming

1. Switch on while holding down one round button. All buttons will flash once when programming mode is started, then release button.
2. Press the button to be programmed. Button will start slow flash.
3. Point the device’s remote control at the Umote window and press the required function. New program will replace any existing program for the button.
4. Button will flash 2 times if setup was successful, 4 times if unsuccessful.
5. Repeat previous 3 steps for other buttons.
6. Switch off to stop programming.

### Program Clear

1. Switch on while holding down both round buttons. All buttons will flash twice when clearing mode is started, then release buttons.
2. Press the button to be cleared.
3. Button will flash 2 times if clearing was successful, 4 times if unsuccessful.
4. Repeat previous 2 steps for other buttons.
5. Switch off to stop clearing.

### Battery Charging

1. Plug mini-USB plug connected to charger into the Umote USB socket.
2. **Red LED** is on while charging, and goes off when fully charged.